---
id: 2026-04-23T10:01:40-0400
title: 2026-04-23 10:01:40
tags:
  - occupational
  - type/minutes
daily: "[[2026-04-23]]"
---
# 2026-04-23 10:01:40

## Virginia Live! Director Review

[[estimating-director-review]] for
[[virginia-live-casino-and-hotel]]:

## Switchgear

Note extensive emergency power provisions
verify control wiring for generator to ATS

#### Lighting HR's

count of circuits, control zones in takeoff notes
lot length

#### Temporary Power

Used two `TEMPORARY POWER - HR`

Narrative
extended light layouts

#### Generator

3000 gallons * 6 dollars per gallon = $18000

#### Labor

ASL Column 2 with adjustments

Site Labor +50%

#### Medium Voltage

Medium voltage cabling downstream of

#### Underground Runs

need rigid 90's for PVC runs 200ft and above

> horizontal? vertical? both?

#### Fixture Labor

Tape light: 1 hour per 6 feet

snap together linear: 1 hour per 5 feet

##### Center Bar Fixture

assuming each crystal is an individual fixture
over 5000 crystals
80 circuits

Arch set A-GAM-442

##### Dragon Fixture

1000 hours

#### Lighting Control

"Networked" to mean either
"Centralized"
or "Standalone" with Network Bridges.

> Wattstopper Network Bridges are limited to 64 devices (zones)

#### DAS

Sold Design Build

#### Historicals

Want to know
casino cost per square foot

#### Composite Cleanup

#### Multi-Shift Impact

20% of hours
add $5 per hour

#### Indirect Labor

16% burden

#### Facade

Extra cost for facade lighting install
250,000

"Go to 150k"
